;BLES00389
;Prince of Persia

:187B080C.DE

[Update CRC32 (Required)]
;set range:0x000000,0x012105
set pointer:eof-3
set range:0x000000,pointer
set [hash]:CRC32
;write at 0x012106:[hash]
set pointer:eof-3
write next (0):[hash]