;BLUS30480
;Toy Story 3

:SAVE

[Update CRC-16 CCITT for SAVE (Required)]
set crc_bandwidth:16
set crc_polynomial:0x1021
set crc_initial_value:0xFFFF
set crc_output_xor:0xFFFFFFFF
set crc_reflection_input:0
set crc_reflection_output:0
;set range:0x0000E4,0x031FFF
set pointer:eof+1
set range:0x0000E4,pointer
set [hash]:crc
write at 0x000064:[hash]